PRESENT STATUS OF SRRCYuen Chung LiuThe 1.3 GeV Taiwan Light Source (TLS) of the Synchrotron RadiationResearch Center (SRRC) located in Hsinchu, Taiwan, ROC has been open tousers for two years since October 1993. The storage ring is operated with a lowemittance lattice at 200 mA initial stored beam current which provides highbrightness light source with photon energy ranging from vacuum ultra violet tosoft x-ray. Up to now, two insertion devices namely the wiggler W20 of 1.8tesla, 25 poles and the undulator U10 with period of 10 cm, 27 poles areinstalled in the storage ring. Presently, there are three high-resolutionVUVphoton beamlines in operation and four x-ray beamlines in acommissioning stage.